Загрузочный сектор для ОС Колибри (FAT12, дискета)

- Описание
  Позволяет загружать KERNEL.MNT с дискет/образов
  объёмом 1.44M, 1.68M, 1.72M и 2.88M
  Для выбора объёма диска, для которого надо собрать
  загрузочный сектор, необходимо в файле boot_fat12.asm
  раскомментировать строку вида:
     include 'floppy????.inc'
  для необходимого объёма диска. Доступные варианты:
  floppy1440.inc,
  floppy1680.inc,
  floppy1743.inc и floppy2880.inc 

- Сборка
  fasm boot_fat12.asm

- Для записи загрузочного сектора на диск/образ под Linux
  можно воспользоваться следующей командой:
  dd if=boot_fat12.bin of=288.img bs=512 count=1 conv=notrunc

---------------------------------------------------------------------

Floppy FAT12 boot sector for KolibriOS.

- Description
   Allows booting KERNEL.MNT floppies/images
   with volumes of 1.44M, 1.68M, 1.72M and 2.88M
   To select the volume of the disk, which should gather
   boot sector, it was necessary in file boot_fat12.asm
   uncomment line:
      include 'floppy????. inc'
   for the necessary disk volume. Available options is:
   floppy1440.inc,
   floppy1680.inc,
   floppy1743.inc and floppy2880.inc

- Compile
  fasm boot_fat12.asm

- To write boot sector to the floppy/image under Linux
  you can use the following command:
  dd if=boot_fat12.bin of=288.img bs=512 count=1 conv=notrunc
